AQUAOX™ KECA 50

|  |  |
| --- | --- |
| **SPECIFICATIONS** | **KECA 50**  |
| Dimensions | 11.08” x 6.4” x 15.2”  |
| Weight | 13 lbs. |
| Power Rating | AC 110V 50/60 Hz |
| Rated Current  | 1.0 A  |
| Water Supply Operating pressure | 14.5 -108 psi |
|  Temperature | 41 - 95° |
| Quantity of generated water  | 3 quart / min. |
| Continuously generated quantity | 132 gallons |
| FAC | 50 (± 10) ppm |
| Ph | 5.0 – 6.5  |